This project corresponds to the 11 taps low-pass FIR filter

shown in slide #9 at the Xilinx Introduction to FIR filters

(but the input string is different from what is shown there)

(https://bit.ly/3Huo7ka) -- implemented in Vitis HLS