This project corresponds to the 6-taps moving average FIR filter with RS232C inputs and outputs as presented in slide #14 at the Xilinx Simple FIR filter examples (<https://bit.ly/3CovdmJ>) -- implemented in Vivado

